; PAR - FILE FOR SIMPLE SLAVE SYSTEM
;
EOPCHR  = 0x7F      ;END OF PRINT CHARACTER
CLSCHR  = 0x5E      ;COMMAND LINE SEPARATOR IS (^)
CLPCHR  = ">"       ;COMMAND LINE PROMPT CHARACTER
SRHDRV  = 0xFF      ;SEARCH FOR COMMANDS ON SYSTEM DRIVE
ATNCHR  = 0x1F      ;ATTENTION CHARACTER IS (^_)
USRSOM  = 0x0D,0x0A,"TurboDOS Rel. 1.41 / 6",0x0D,0x0A,0x0A,"$"
SLRCHR  = 0x1E      ;SLAVE RESET CHARACTER IS (^^)
COMPAT  = 0xB0      ;COMPATIBILITY FLAGS: PERMISSIVE, MIXED MODE, GLOBAL WRITE
WARMFN  = 0,"WARMSTRT","186" ;WARMSTART AUTOLOAD FILENAME FOR 16 BIT SLAVE 
OSMLEN  = (0xFFF)   ;LENGTH OF DYNAMIC WORKING STORAGE
OSMTOP  = (0xFA0)   ;TOP OF MEMORY FOR DYNAMIC WORKING STORAGE (64KB)
MEMTBL  = 0x01,(0x0060),(0x3F9F) ;MEMORY SIZE 256KB
CONAST  = 1,CONDRA  ;CONSOLE ASSIGNMENT TABLE (CHANNEL B)
CONBR   = 0x8F      ;CONSOLE BAUDRATE
CONIND  = 0xC2      ;CONSOLE PROTOCOL CCTXX
PTRAST  = 0x80,(0),0x81,(0),1,LSTDRA ;PRINTER ASSIGNMENT TABLE LOCAL PRINTER C
PRTMOD  = 0         ;PRINTING DIRECT
QUEPTR  = 3         ;TO LOCAL PRINTER C
;PATCH 2 - TO MAKE OPTIMIZED CONSOLE STATUS FUNCTIONS TO RETURN
;          STATUS IN L-REG (AS WELL AS A-REG).
CINTRY + 0X41 = 0XE9,[PATCH]
PATCH = 0X31,0XC0,0X89,0XC3,0XC3
;PATCH 3 - TO CORRECT HANG-UP AFTER UNSUCCESSFUL PROGRAM LOAD.
PLFCN + 0X39 = [PATCH+0X05]
PATCH + 0X05 = 0XC7,0X06,BASPAG-0X128,0X00,0X00,0XE9,[INCMOB]
;PATCH 13 - TO CORRECT PROBLEMS IN T-FUNCTION 41 EXPLICIT NETWORK ROUTING.
NETREQ + 0X477 = 0X3C,0XFE,0X74,0X28,0XD0,0XC8,0XD0,0XC8,0XD0,0XC8,0XD0,0XC8
                 0X24,0X0F,0X74,0X34
NETREQ + 0X4AA = 0XE9,[NETREQ+0X49C]
GSX86 + 0x61 = 0x1B,0x3D,0x20,0x40,0x1B,0x47,0x44,"    PMU 186    ",0x1B,0x47,0x40,0x0D,0x0A,"$"
ROUFCN + 0x15 = 0xD1,0x06
GSX86 = 0xFF
COLDST + 0x55 = 0x90,0x90,0x90
COLDST + 0x59 = 0x90,0x90,0x90
COLDST + 0x5F = 0x90,0x90,0x90
COLDST + 0x63 = 0x90,0x90,0x90
COLDST + 0x69 = 0x90,0x90,0x90
