
	*****************************************************************************
	*                                                                           *
	*          S T R E A M E R   B A C K U P   S E T   D I R E C T O R Y        *
	*                                                                           *
	*                                  ( Release 7 )                            *
	*                                                                           *
        *****************************************************************************

	Description:
	-----------
		The command SDIR gives a directory survey of a streamer tape
		backup set. If all parameters are specified, it works in
		batch mode, otherwise in interactive mode. Optionally the
		output may be printed.
		For performance reasons the program creates a file BACKUP.DIR
		on the default disk drive, which contains a "compressed"
		directory and which is not deleted after program run.
		SDIR has to be started by a privileged user in the Master. 
		The program requires TurboDOS release 1.4 with P3000 release 7.
	_____________________________________________________________________________

	Example:
	-------
		0A>SDIR 13:*.CMD;L         (L = protocol option)

		Streamer Tape Backup Set Directory  (Release 7)       Date: 07 Jul 86
		Mount streamer tape BACKUP.*00 (CR continue,^C abort) 

		BACKUP.000        13:*       .CMD         5 FILES       76K DISPLAYED
		---------------------------------------------------------------------
		COPY    .CMD    8K       DRIVE   .CMD    4K       SAVESTR .CMD    56K
		DELETE  .CMD    4K       DUMP    .CMD    4K


		0A>SDIR
		Streamer Tape Backup Set Directory  (Release 7)       Date: 07 Jul 86
		Mount streamer tape BACKUP.*00 (CR continue,^C abort) 

		User number (0 - 31)  or  ?   : ?

		Non-empty user areas:  0  .  .  .  4  .  6  .  .  .  .  .  . 13  .  .
		                      16  .  .  .  .  .  .  .  .  .  .  .  .  .  . 31

		User number (0 - 31)  or  ?   : 13
		File name (wild cards allowed): *.CMD

		BACKUP.000        13:*       .CMD         5 FILES       76K DISPLAYED
		---------------------------------------------------------------------
		COPY    .CMD    8K       DRIVE   .CMD    4K       SAVESTR .CMD    56K
		DELETE  .CMD    4K       DUMP    .CMD    4K

		User number (0 - 31)  or  ?   : ^C

	_____________________________________________________________________________

	Error messages:
	--------------
		Program not executed on master
		Backup set directory empty
		BACKUP.DIR cannot be created on volume
		BACKUP.DIR cannot be opened on volume
		Write error on BACKUP.DIR on volume
		Read error on BACKUP.DIR on volume 
		Streamer tape drive not available
		Read error on backup set directory
		Read/write error on backup volume label (Retry,Abort) 
		No backup set on streamer tape		
		Wrong streamer tape mounted
		Streamer tape drive not ready
		Tape qualification error
		Irrecoverable error on streamer tape, drive status = 
	_____________________________________________________________________________

	Turnover:
	--------
		SDIR.CMD		(07 Jul 86)
	_____________________________________________________________________________
